Building the Network You Need with OpenBSD's PF: BSDCan, Ottawa May 6th, 2009
Prev |  | Next

# Wireless networks made easy

Check your dmesg

    ath0 at pci1 dev 4 function 0 "Atheros AR5212" rev 0x01: irq 11
    ath0: AR5212 5.6 phy 4.1 rf5111 1.7 rf2111 2.3, ETSI1W, address
    00:0d:88:c8:a7:c4

Access point, OpenBSD `/etc/hostname.ath0`:

    up media autoselect mediaopt hostap mode 11b chan 6 nwid unwiredbsd \
     nwkey 0x1deadbeef9
    inet 10.168.103.1

From OpenBSD 4.4 onwards, we have WPA