Building the Network You Need with OpenBSD's PF: BSDCan, Ottawa May 6th, 2009
Prev |  | Next

# You're wondering ... Learn BSD?

I Know Some Linux, but I Need to Learn Some BSD. Any Pointers?

- Network interface name equals driver name + sequence number, such as `xl0` (3Com), `em0`, `fxp0` (Intel), and so on

- Configuration centralized in `/etc/rc.conf`, on OpenBSD you create, edit `/etc/rc.conf.local` to override `rc.conf` defaults

- PF is configured via `/etc/pf.conf` and command line - pfctl(8)